15“ 3-WAY POWERED SPEAKER

1) 용  도

본 기기는 15“ 3-WAY 풀 레인지 파워드 스피커로서 최고의 음질이 필요한 강당, 소공연장 등 사용이 가능하다. 고품질의 CLASS-D 디지털 파워 앰프가 내장되어 있으며 사용자가 시스템을 최적화 할 수 있도록 선택 가능한 두 개의 EQ를 제공한다. 또한, ON-BOARD의 DSP, EQ는 무선 WI-FI를 통해 제어할 수 있다. 퍼포먼스시 최대의 성능을 구현할 수 있도록 사이즈, 무게 등을 고려하여 디자인된 컴팩트형 스피커이다.

2) 기  능

- 디퍼렌셜 드라이브 기술 적용

- 듀얼 15인치 저음역대 드라이버로 낮은 노이즈 및 높은 SPL 제공

- 고품질 CLASS-D 파워 앰프 내장

- 무선 WI-FI를 통한 DSP, EQ 제어

- 90 ° x 50 °의 커버리지

3) 사  양

- System type : Self Powered 15”, Three-way, bass-reflex

- Frequency Range (-10dB)	: Normal 35Hz ~ 20kHz

: Boost 34Hz ~ 20kHz

- Frequency Response (-3dB)	: Normal 42Hz ~ 20kHz

: Boost 39Hz ~ 20kHz

- Input impedance : 20K ohms (Balanced), 10K ohms (Unbalanced)

- Dynamic Control : dbx type IV™ limiter circuit

- Power amp design : Highly etticient Class-D amp

- Coverage : 90 x 50 deg.

- Crossover frequencies : 2.1 kHz

- Power rating	: 1500W cont. (750W x2)

- Directivity index (DI) : 10.5 dB

- Directivity factor (Q) : 11.2

- Max SPL : 138 dB Peak

- Transducers : LF 15“, MF 6.5”, HF 1.5”

- Finish : Obsidian DuraFlex™ finish

- Connectors : 2 x Balanced XLR, 2 x Unbalanced RCA

- Power input : 100V ~ 240V, 50/60Hz

- Dimension (H x W x D)mm : 938 x 446 x 539

- Weight : 32.38 kg