STAGE MONITOR SPEAKER (PRX325D)

1) 용  도

본 기기는 라이브 공연 및 무대 모니터링을 위해 디자인된 듀얼 15“ 2-WAY 스피커 시스템이다. 상단 우퍼는 중음역과 저음역, 하단 우퍼는 저음에 중점을 두며 이러한 3-WAY 디자인은 추가적인 서브 우퍼 스피커 없이도 시스템에 저음대역을 제공한다. 티타늄 다이어프램이 장착된 15” 압축 드라이버는 깨끗하고 따뜻한 고음과 안정성을 제공한다. JBL SonicGuard ™ 기술은 고주파수 드라이버를 과도한 전력으로부터 보호하여 시스템의 안정성을 향상시킨다. 정밀한 크로스오버는 두 개의 드라이버에 오버랩을 최소화하며 명확한 컷 주파수를 공급한다.

2) 기  능

- 단단하고 풍부한 저음, 고효율의 프리미엄 듀얼 15인치 로우 드라이버

- 티타늄 다이어프램이 장착된 1인치 강 유체 냉각 압축 드라이버로 깨끗하고 따뜻한 고음과 안정성 제공

- JBL SonicGuard ™ 기술은 고주파 드라이버를 과도한 전력으로부터 보호

- 정밀하게 제작 된 크로스 오버 피드로 선명한 주파수로 드라이버를 공급

- Progressive Transition™ 웨이브가이드는 우수한 커버리지 제어, 왜곡 감소 및 부드러운 주파수 응답 제공

- 찌그러짐 방지 그릴은 이동 또는 공연 중 내부 손상을 방지

3) 사  양

- System Type : Dual 15” 2-way speaker

- Frequency Range (-10 dB) : 35 Hz – 16 kHz

- Frequency Response (±3dB) : 45 Hz – 12 kHz

- Sensitivity (1w@1m) : 100 dB SPL

- Nominal Impedance : 4 Ω

- Power Capacity : 500 W

- Peak Power Capacity : 2000W

- Maximum SPL : 133 dB

- Nominal Dispersion : 90° × 50°

- Crossover Frequency : 2 kHz

- HF Driver : JBL 2412 1” exit compression driver mounted on Progressive Transition TM Waveguide

- LF Driver : 2 × JBL M115-8A

- Input Connector : Parallel Neutrik Speakon® NL-4 (×1)；1/4” TS phone jack (×1);

- Enclosure Construction : 15 mm (0.6 in) MDF (Medium Density Fiberboard) with glued
and mechanically fastened joint detail; black painting.

- Mounting & Suspension : No suspension points. For ground standing

- Dimensions (H×W×D) : 1075× 454× 467 mm

- Weight: 37.4 kg