HDMI 4K INPUT BOARD (DGX-I-HDMI-4K)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 4K UHD HDMI 입력 보드이며, 4개의 HDMI 포트가 오디오, 비디오 신호 전송을 지원한다.

2) 기  능

- 4K UHD 비디오 지원

- InstaGate Pro® HDCP 인증키 기술

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 오디오 지원

3) 사  양

GENERAL

- Compatible AMX Products:

Must be used in conjunction with an Enova DGX 800, 1600, 3200 or 6400 Digital Media Enclosure

- Regulatory Compliance:

See Enova DGX Digital Media Switcher Enclosure for regulatory compliance

- Recommended Accessories

CBL-HDMI-FL2-16, HDMI 4K60 MyTurn Ready Flat Cable, 16 Feet (FG10-2192-16)

CBL-HDMI-FL2-32, HDMI 4K60 MyTurn Ready Flat Cable, 32 Feet (FG10-2192-32)

HDMI w/HDCP

- Compatible Formats: HDMI, HDCP, DVI

- Signal Type Support:

HDMI

DVI-D (Single Link With HDMI Cable Adapter)

DisplayPort ++ (Input Only, With HDMI Cable Adapter)

- Connectors: 4 HDMI Type A Female Ports

- Video Data Rate (Max): 8.91 Gbps (max)

- Video Pixel Clock (Max): 297 MHz

- Progressive Resolution Support:

480p up to 4096x2160p,60 Hz (Y/Cb/Cr 4:2:0 & 4K RX Scaler in Bypass)

- Interlaced Resolution Support:

480i, 576i, 1080i (NOTE: If input is interlaced, all scaled outputs will deinterlace video to a progressive resolution format. If in scaler Bypass mode interlaced input will pass through unaltered.)

- 4K Resolution Support:

3840x2160p@24/25/30 Hz, 4096x2160p@24/25/30 Hz, 3840x2160p@60 Hz, 4:2:0*, 4096x2160p@60 Hz, 4:2:0 (NOTE: Supported by DX-RX-4K when in Bypass Scaling mode.)

- HDMI Cable Requirement: HDMI High Speed Cable, Category 2, Required

- Input Equalization:

Yes, adaptive to 21 ft. (7 m) (Cable distance support dependent on cable quality and signal format.)

- Input Re-clocking (CDR): Yes

- Deep Color Support:

24-bit, 30-bit, 36-bit

30-bit and 36-bit are only supported when the HDMI Output Board or DXLink RX Scaler is in Bypass mode and format is 1080p60 or less.

- Color Space Support:

RGB 4:4:4

YCbCr 4:4:4, 4:2:2, and 4:2:0

Input signal support for YCbCr 4:4:4 and 4:2:2, output color-space is converted to RGB 4:4:4

4:2:0 only supported at 2160p 50/60 Hz with 4K RX Scaler in Bypass

- 3D Format Support:

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/60 Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

NOTE: The Scaler on corresponding output board or RX must be set to Bypass mode.

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192 kHz

- Local Audio Support: Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel

- Audio Switching Board Support:

Supports break-away audio switching of 2 CH L-PCM for all channels

Supports downmix from one input channel of Dolby True-HD, Dolby Digital, DTS-HD, DTS, or 2 to 8 channel L-PCM

- DDC/EDID Support:

EDID provided by Enova DGX Digital Media Switcher to the digital (HDMI) input on the DXLink Transmitter

EDID is user re-programmable

- HDCP Support: Yes, full matrix HDCP 1.4 support (includes any input to any or all outputs)

Key Management System

- AMX HDCP InstaGate Pro Technology:

Key support up to 16 devices per output, independent of source device

- CEC Support: None

- Input Propagation Delay: 2 us

- Connectors: 4 HDMI Type A Female Ports