VIDEO ENCODER (NMX-ENC-N1134A)

1) 용  도

본 기기는 아날로그 신호를 디지털 신호로 바꾸어 주는 비디오 인코더로서, 기가비트 이더넷 네트워크를 통해 컨트롤, HDMI, AUDIO 신호를 전송할 수 있다. 또한 4K 및 UHD의 고화질 해상도를 수용하고 PoE +를 통해 전원과 신호를 동시에 전달할 수 있으며 설치가 간단하다.

2) 기  능

- SDI-HDMI 변환기 없이 SDI 소스 비디오 배포

- 60fps / 10ms 서브 프레임 대기 시간

- MCP (Minimal Proprietary Compression) 알고리즘 – 압축 최소화

- PoE 전원 공급

- 기본 NetLinx

3) 사  양

- PORTS

- IR:2-pin terminal Phoenix connector

- RS232: 3-pin terminal Phoenix connector which provides a serial control interface.

- AUDIO: 5-pin terminal Phoenix connector which provides user-selectable balanced/unbalanced input. - Dedicated audio input

- HD-SDI In: BNC

- HD-SDI Out: BNC for HD-SDI pass through

- VGA IN: DB15 analog input

- USB connectors (front panel): USB-B control input and two USB-A control inputs

- ENVIRONMENTAL

- Temperature: 32° to 104°F (0° to 40°C)

- Humidity: 10% to 90% RH (non-condensing)

- Heat Dissipation: Up to ~44 BTU/hr

- GENERAL

- Dimensions (HWD): 1.05” x 7.888” x 5.5” (2.67 cm x 20.04 cm x 13.8 cm)

- Weight: 1.55 lbs (0.7 kg)