EQUALIZERS (1231)

1) 용  도

본 기기는 신호의 증폭이나 전송 과정에서 생기는 변형을 보정하기 위하여 증폭 및 균일화 기능을 제공하고  아날로그 스타일의 인터페이스에서 볼 수 있는 장점들과 디지털 프로세서에서의 장점들을 결합시킨 프로세서로서, 탁월한 사운드와 견고한 안정성을 제공하여 최상의 사운드를 보장한다. 또한 두 개의 1/3옥타브 31밴드 채널, 옥타브 로우 컷 필터 당 전환 가능한 40Hz / 18dB,  선택 가능한  ±6dB 또는 ±15dB 부스트 / 커팅 범위, Chassis /Signal 그라운드 리프트 능력, 내부 파워 서플라이 트랜스포머, 파워 오프 하드와이어 릴레이 바이패스 (2초 파워 업 딜레이를 가짐)와 같은 뛰어난 기능을 가지고 있다.

2) 기  능

- 전환 가능한 부스트

- 컷 범위 ±6 또는 ±15dB

- RF 필터링된 입력 및 출력

- XLR, Barrier Strip, and 1/4" TRS connectors

- ±12dB 입력 게인 범위

- 18dB / octave 40Hz Bessel 로우 컷 필터

- 섀시 / 신호 그라운드 리프트 기능

- 내부 전원 공급 장치 변압기

3) 사  양

- In/output channel : 2in/2out

- Input Connectors : 1/4" TRS, female XLR (pin 2 hot), and barrier terminal strip

- Input Type : Electronically balanced/unbalanced, RF filtered

- Input Impedance : Balanced 40k ohm, unbalanced 20k ohm

- Max Input : >+21dBu balanced or unbalanced

- CMRR : >40dB, typically >55dB at 1kHz

- Output Connectors : 1/4" TRS, male XLR (pin 2 hot), and barrier terminal strip

- Output Type : Impedance-balanced/unbalanced, RF filtered

- Output Impedance : Balanced 200 ohm, unbalanced 100 ohm

- Max Output : >+21dBu balanced/unbalanced into 2k ohm

- THD+Noise : <0.005%

- Frequency Response : <10Hz to >50kHz, +0.5/-3dB

- Power Consumption : 24W

- Dimension (H x W x D)mm : 134 x 483 x 201

- Weight : 4.81 kg