BATTERY-OPERATED PHANTOM POWER SUPPLY & MINI RECORDING MIXER (B23L)

1) 용  도

본 기기는 9V 팬텀 전원을 공급하는 소형 전원 공급 장치로서, 2개의 미니 XLR-F 입력 (L 및 R)을 통해 최대 2개의 마이크에 사용이 가능하다. 또한 모노 또는 스테레오 모드로 전환가능하며 2개의 AA배터리 사용으로 평균 30시간으로 사용이 가능하다.

2) 기  능

- 9V 팬텀 전원 공급

- 소형 전원 공급 장치

- 2개의 미니 XLR-F 입력

- 모노 또는 스테레오 모드로 전환가능

3) 사  양

- Frequency Response : 20 Hz - 20 kHz

- Input Channels : Two mini XLR inputs

- Output Channels : 3.5 mm stereo output jack (max. 55 VDC)

- Max Input Level : 0 dBV

- Max Output Level Stereo Line : 0 dBV +/- 1 dB @ 1 kHz < 0.1 %

- Max Output Level Stereo Mic : 0 dBV +/- 1 dB @ 1 kHz < 1 %

- Input Impedance : 5 kohms

- Output Impedance : 200 ohms unbalanced

- Noise Line (Mono & Stereo) : < 5 uV (A)

- Noise MIC (Mono & Stereo) : < 22 uV (A)

- Power Supply : Two AA alkaline or rechargeable batteries

- Phantom Voltage : 9 V (open loop), 4 V (at 4,2 kOhm)

- Power Consumption : 40 mA @ 3 VDC (line mode)

- Lifespan of the Batteries : 30 - 50 h, depends on the battery capacity

- Temperature Range : -10 °C – 60 °C (14 °F - 140 °F)

- Dimension (H x W x D)mm : 89 x 70 x 26

- Net Weight : 115 g