EXTENSION LINE ARRAY COLUMN LOUDSPEAKER

1) 용  도

본 기기는 저음대역의 보강을 위한 익스텐션 스피커로써, BeamWidth 기술이 적용되어 있는 스피커이다. 본 스피커는 슬림형 디자인이 필요한 공간에 최적화된 스피커이며, 보이스에 대한 명료도를 한층 증대하였다.

2) 기  능

- 인테리어와 최적의 조화

- Constant Beamwidth 기술 탑재

3) 사  양

CBT70JE-1

- System type : Extension Column line-array speaker

- Frequency Range (-10dB) : 45Hz ~ 700Hz

- Components : 5“x4 LF

- Power rating	: 500W cont. (PEAK 2000W)

- Sensitivity(1W@1m) : 90dB

- Max SPL : 117dB

- Impedance : 8 ohm

- Weight : 8.2kg

CBT70J-1

- System type : 2- WAY Column line-array speaker

- Frequency Range (-10dB) : 60Hz ~ 20kHz

- Components : 5“x4 LF , 1”X16 HF

- Coverage	: narrow mode 150 x 25 deg.

: broad mode 150 x 45 deg.

- Power rating	: 500W cont. (PEAK 2000W)

- Sensitivity(1W@1m)	: narrow speech mode 98 dB

: narrow music mode 93 dB

: broad speech mode 96 dB

: broad music mode 92 dB

- Max SPL	: narrow speech mode 125dB (peak 131dB)

: narrow music mode 120 dB (peak 126dB)

: broad speech mode 123 dB (peak 129dB)

: broad music mode 119 dB (peak 125dB)

- Impedance : 8 ohm

- Enclosure : Fiberflass reinforced ABS cabinet

- Outdoor Capability : IP-55 (IEC529 구성 필요)

- Dimension (H x W x D)mm : 694 x 170 x 237

- Weight : 9.5kg