EQUALIZERS (215s)

1) 용  도

본 기기는 신호의 증폭이나 전송 과정에서 생기는 변형을 보정하기 위하여 증폭 및 균일화 기능을 제공하는 이퀄라이저로서, 탁월한 사운드와 견고한 안정성을 제공하여 최상의 사운드를 보장한다. 또한 두 개의 1/3옥타브 15밴드 채널, ±12dB 입력게인, 전환가능 ±6dB 또는 ±12dB 부스트 / 커팅범위, 직관적인 사용자 인터페이스 및 출력 레벨 미터링, 간편한 컨트롤을 제공한다.

2) 기  능

- 듀얼 15 밴드

- 1/3 옥타브 Constant Q 주파수 대역

- 전환 가능한 부스트 / 컷 범위 ±6 또는 ±12dB

- 전면 패널 바이 패스 스위치

- ±12dB 입력 게인 범위

- 출력 레벨 모니터링을 위한 4 분할 LED 래더

- XLR 및 TRS 입력 및 출력

- 10Hz 에서 50kHz의 주파수 응답

- 108dB 이상의 다이나믹 레인지

3) 사  양

- In/output channel : 2in/2out

- Input Connectors : 1/4" TRS, female XLR (pin 2 hot)

- Input Type : Electronically balanced/unbalanced, RF filtered

- Input Impedance : Balanced 40k ohm, unbalanced 20k ohm

- Max Input : >+21dBu balanced or unbalanced

- CMRR : >40dB, typically >55dB at 1kHz

- Output Connectors : 1/4" TRS, male XLR (pin 2 hot)

- Output Type : Impedance-balanced/unbalanced, RF filtered

- Output Impedance : Balanced 100 ohm, unbalanced 50 ohm

- Max Output : >+21dBu balanced/unbalanced into 2k ohm

- THD+Noise : <0.003%

- Frequency Response : <10Hz to >50kHz, +0.5/-3dB

- Power Consumption : 15W

- Dimension (H x W x D)mm : 44 x 482.6 x 152.4

- Weight : 2.2 kg