CROSSOVERS (223xs)

1) 용  도

본 기기는 정밀 필터를 사용하여 오디오 신호를 분리하고 다른 신호간의 주파수를 라우드 스피커 드라이버로 전달하는 dual channel crossover 프로세서로서, 레벨 매칭, 출력 위상 반전, 40Hz 로우 컷 필터 및 저주파 출력을 위한 독립적 인 출력 게인 컨트롤를 가지고 있으며, 밸런스형 XLR 입력과 출력을 제공한다. 공연 동안 어떤 설정에서의 돌발적인 변화를 막기 위해서, 컨트롤 부분 중 몇 가지는 뒷면 패널에 위치에 있다. 또한, 스테레오 2웨이나 3-way의 2개의 모드를 가지고 있고, 뒤 패널에 설치된 스위치들은 양 채널에 대해 크로스오버 주파수 범위를 개별적으로 선택 할 수 있다.

2) 기  능

- XLR 밸런스 인 / 아웃

- 스테레오 2 웨이 또는 모노 3웨이 조작을 위한 모드 스위치

- 두 채널의 x10 range 스위치

- 40Hz 하이패스 (로우 컷) 필터

- 모든 출력에서 위상 반전 스위치

- 모든 출력에 대한 개별 레벨 컨트롤

- 스테레오 / 모노 상태 LED

3) 사  양

- In/output channel : 2in/4out

- Input Connectors : XLR (pin 2 hot)

- Input Type : Electronically balanced/unbalanced, RF filtered

- Input Impedance : Balanced >50k ohm, unbalanced >25k ohm

- Max Input : >+22dBu balanced or unbalanced

- CMRR : >40dB, typically >55dB at 1kHz

- Output Connectors : XLR

- Output Type : Impedance-balanaced/unbalanced, RF filtered

- Output Impedance : Balanced 200 ohm, unbalanced 100 ohm

- Max Output : >+21dBu balanced/unbalanced

- THD+Noise : < 0.004% at +4 dBu, 1 kHz; < 0.04% at +20 dBu, 1 kHz

- Frequency Response : < 3 Hz to > 90 kHz, +0/-3 dB

- Power Consumption : 15W

- Dimension (H x W x D)mm : 44 x 483 x 175

- Weight : 1.7 kg