PERSONAL MONITOR CONTROLLER

1) 용  도

본 기기는 연주자가 모니터 믹스를 직접 할 수 있도록 해주는 리모트 컨트롤로서, 16개 채널을 믹스할 수 있다, 또한 셋업 기능을 내장하여 빠르게 셋업할 수 있으며, 각 채널 별로 PAN, 이펙트(리버브), 톤, 레벨 등을 조정하여 16개의 프리셋에 저장할 수 있다. 각 컨트롤러 스테이션별로 리버브가 기본 내장되어 있어 실시간으로 각 연주자의 취향에 맞추어 리버브를 사용할 수 있다. 또한 헤드폰, 인이어 모니터 뿐만 아니라 모든 모니터 스피커와 함께 사용 가능하다.

2) 기  능

- 16채널 퍼스널 모니터 리모트 컨트롤러

- 빠르고 쉬운 셋업

- 리버브 이펙터

- 리미터 내장

- 16개 프리셋 저장

- USB 를 사용한 손쉬운 펌웨어 업데이트

- LCD 스크린

- BLU-Link 네트워크 오디오 사용

- 견고한 마이크 스탠드 용 마운트

- 48kHz/96kHz 전환 가능한 D/A 컨버팅

- 컨트롤과 음질에서의 손실 없이 60개 유닛의 동시 사용 가능

3) 사  양

- Frequency Response : +0/-0.2 dB 20 Hz – 20 kHz

- Dynamic Range : >108 dB unweighted 22 Hz – 22 kHz bandwidth >112 dB A-weighted

- Bit-Depth : 24-bit

- Sample Rate : 48 kHz or 96 kHz

- Connectors : 2 x RJ45 Ethernet connectors

- Maximum Cable Length : 100 m/328 ft between devices (Category 5e cable)

- Analog Outputs : XLR & 1/4”

- Maximum Output Level : 20 dBu

- Output Impedance : 40 Ω

- Headphone Outputs : 1/8” & 1/4”

- Power/Impedance : 900 mW per channel at 50 Ω (1/8” and 1/4” jacks are in parallel)

- Power Consumption : 18W

- Power Requirements : 9 V DC 2.0 A

- Dimension (H x W x D)mm : 21 x 115 x 413

- Weight : 2.2 kg