POWERED LINE-ARRAY SPEAKER

1) 용  도

본 기기는 렌탈 하우스, 투어링 아티스트, DJ 및 고정설치 등 중/대형 공간을 위한 컴팩트형 파워드 라인어레이 스피커이다. 내장된 DSP 및 앰프는 플러그 앤 플레이 환경을 제공하는 동시에 전 세계 어디에서나 일관성과 최적의 성능을 제공한다. JBL 트랜스듀서와 새로운 음향 디자인은 뛰어난 사운드와 동급 최고의 최대 SPL을 제공한다. 듀얼 10“ 네오디뮴 디퍼렌셜 드라이브 우퍼와 3” 압축 드라이버로 구성되어 있다. PC에 최적화된 인클로저는 복합 재료로 만들어졌으며 컴팩트하고 가벼우며 우수한 성능을 제공한다. 혁신적인 3포인트 리깅 시스템과 액세서리를 통해 다양한 방식으로 설치 및 확장하여 사용한다. Windows, macOS, iPAD OS를 포함한 여러 플랫폼에서 시스템을 설계, 제어, 관리할 수 있다.

2) 기  능

- 운송, 보관, 리깅에 최적화된 고성능, 고밀도 시스템 솔루션

- 낮은 왜곡, 높은 충실도, 동급 최고 출력을 제공하는 고출력 트랜스듀서

- 범용 전원 공급 장치가 탑재된 수동 냉각 CLASS D 앰프

- Neutrik etherCON 커넥터가 탑재된 듀얼 이더넷 포트

- Harman HControl 이더넷 프로토콜 지원

- 사용자 제어 가능한 DSP

- LevelMax 리미팅은 트랜스듀서 보호를 위해 정교한 excursion-control 알고리즘 사용

- 후면 패널의 LCD는 제어 기능에 대한 완벽한 액세스 제공

- 강화된 복합 라우드스피커 인클로저

- 혁신적인 3포인트 리깅 시스템

3) 사  양

- System Type : Line Array, two-way active

- Frequency Range (-10dB) : 53Hz ~ 19kHz

- Frequency Range (-3dB) : 60Hz ~ 18kHz

- Horizontal Coverage : 105 deg.

- Maximum Peak Output : 135 dB

- Transducers : LF 2x10“, HF 1x3“

- Amp Type : Class-D

- Amp Power : 600W Continuous (LF 400W / HF 200W)
880W Peak (LF 580W / HF 300W)

- DSP Sample Rate / Bit Depth: 48kHz / 24bit

- Networking Type : TCP/IP

- AC Power Voltage Range : 100-240 VAC, 50/60Hz

- IP Rating : IP54

- Inter-enclosure Angle : 0.5, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12

- Connectors : 2x Neutrik XLR (IN/OUT)
2x Neutrik etherCON®
2x (IN/OUT) Neutrik powerCON TRUE1 TOP®

- Dimension (H x W x D)mm : 305 x 716 x 519

- Weight : 26.7 kg