DIGITAL POWER AMPLIFIER

1) 용  도

본 기기는 오디오 믹서로부터 전달된 오디오 신호를 스피커가 구동될 수 있는 전압의 크기로 증폭하는 기기로서 강하고 가벼우며 투어링 사운드 어플리케이션 사용에 편리하다. 특허인 Class-I 출력회로는 High Efficiency의 우수한 사운드와 높은 출력을 제공한다. 24bit, 96kHz 의 컨버터와 DSP가 내장되어 있어 효율적인 사용과 관리에 이상적인 디지털 앰프이다. 또한 스피커에 대한 전용 프리셋과 EQ, DELAY 등 다양한 효과를 적용할 수 있어 최적의 음향 효과를 제공할 수 있다.

2) 기  능

- 컬러 QVGA 디스플레이

- IIR 필터 및 FIR선형 위상 필터를 지원하는 BSS 옴니드라이브 HD DSP 프로세싱

- 어떤 상황에도 최대의 파워를 제공하는 PFC(전력 효율 교정)방식의 글로벌전원 공급기

- 아날로그, AES/EBU, 코브라넷, 이더넷 연결을 동시에 제공하는 유일한 제품

- LevelMAX 피크 전압, RMS 파워, 열 변환 리미터가 동시에 작동하여 부드럽고 정확한 응답성과 보다 나은 소리 및 높은 SPL을 보유

- HiQnet 소프트웨어로 모니터링 가능

3) 사  양

- Channels : 2 input, 2 output

- Power output	: 2-ohm (per ch), 3,750W

: 4-ohm (per ch), 4,500W

: 8-ohm (per ch), 2,100W

: 4-ohm Bridge, 7,500W

: 8-ohm Bridge, 9,000W

- Input Sensitivity : 1.4Vrms to 7.75Vrms

- Signal to Noise Ratio (A-weighted) : > 112 dB

- T.H.D : < 0.1%

- Frequency Response : ± 0.25dB

- Intermodulation Distortion (IMD) : < 0.2%

- Crosstalk : > 80 dB

- Common Mode Rejection (CMR) : > 70 dB typical

- Dimensions (H x W x D) : 89 x 483 x 411 mm

- Weight : 12.7 kg