STAGE MONITOR SPEAKER (PRX315D)

1) 용  도

본 기기는 라이브 공연 및 무대 모니터링을 위해 디자인된 15“ 2-WAY 스피커 시스템이다. 견고한 저음, 고효율 및 고출력을 제공하며 티타늄 다이어프램이 장착된 15” 압축 드라이버는 깨끗하고 따뜻한 고음과 안정성을 제공한다. JBL SonicGuard ™ 기술은 고주파수 드라이버를 과도한 전력으로부터 보호하여 시스템의 안정성을 향상시킨다. 정밀한 크로스오버는 두 개의 드라이버에 오버랩을 최소화하며 명확한 컷 주파수를 공급한다.

2) 기  능

- 견고하고 풍부한 저음, 고효율의 프리미엄 15인치 로우 드라이버

- 티타늄 다이어프램이 장착된 1인치 강 유체 냉각 압축 드라이버로 깨끗하고 따뜻한 고음과 안정성 제공

- JBL SonicGuard ™ 기술은 고주파 드라이버를 과도한 전력으로부터 보호

- 정밀하게 제작 된 크로스 오버 피드로 선명한 주파수로 드라이버를 공급

- Progressive Transition™ 웨이브가이드는 우수한 커버리지 제어, 왜곡 감소 및 부드러운 주파수 응답 제공

- 찌그러짐 방지 그릴은 이동 또는 공연 중 내부 손상을 방지

3) 사  양

- System Type : 15” 2-way speaker

- Frequency Range (-10 dB) : 38 Hz – 16 kHz

- Frequency Response (±3dB) : 50 Hz – 12.5 kHz

- Sensitivity (1w@1m) : 98 dB SPL

- Nominal Impedance : 8 Ω

- Power Capacity2 : 250 W

- Peak Power Capacity2 : 1000 W

- Maximum SPL: 128 dB

- Nominal Dispersion : 90° × 50°

- Crossover Frequency : 1.6 kHz

- HF Driver : JBL 2412 1” exit compression driver mounted on Progressive TransitionTM Waveguide

- LF Driver : JBL M115-8A

- Input Connector : Parallel Neutrik Speakon® NL-4 (×1)；1/4” TS phone jack (×1);

- Enclosure Construction : `15 mm (0.6 in) MDF (Medium Density Fiberboard) with glued
and mechanically fastened joint detail; black painting

- Grille : 18-gauge, powder-coated steel

- Mounting & Suspension : 36 mm, dual-angle pole-mount socket; 12×M10 suspension points

- Dimensions (H×W×D) : 681× 455 × 422 mm

- Weight : 23.9 kg