LOUDSPEAKER (CV1270)

1) 용  도

본 기기는 12“ 2-WAY 풀레인지 라우드 스피커로써 레스토랑, 카페 회의실, 홀 등 다양한 사이트에 설치가 가능하다. 100°×70°의 부드럽고 균일한 커버리지를 제공하며 패시브 네트워크는 오버랩 대역을 최소화한다.

2) 기  능

- 12 인치 고효율 우퍼 디자인

- 1” 폴리머 다이어프램 압축 드라이버

- 파우더 코팅 1.5mm 스틸 그릴

- 15mm 합판으로 제작된 인클로저

- 100 °×70 ° 커버리지 패턴

- 최적의 드라이버 통합을 위한 정밀한 엔지니어링 크로스 오버

3) 사  양

- System Type : 12”, 2-way, bass-reflex

- Frequency Range (-10 dB) : 48 Hz – 20 kHz

- Frequency Response (±3 dB) : 80 Hz – 18 kHz

- System Sensitivity (1w @ 1m) : 96 dB

- Nominal Impedance : 8 Ω

- Maximum SPL (1m) : 122 dB continuous average (128 dB peak)

- Power Rating (Continuous/Program/Peak) : 350 W/700 W/1400 W

- Coverage : 100° × 70° (H × V)

- LF Driver : 1 x 12” woofer

- HF Driver : 1 x 2414H-C tweeter

- Enclosure : Trapezoid, 15 mm plywood

- Suspension : 15 × M10 threaded suspension points

- Color : Textured paint, black. White (-WH) available upon request.

- Enclosure Construction : Powder coated 1.5mm perforated cold rolled steel

- Input Connector : Dual NL4MP Neutrik Speakon® in parallel for loop-through

- Dimensions (H×W×D) : 600 × 370× 392 mm

- Weight : 18.2 kg