LOUDSPEAKER (CV3015/99)

1) 용  도

본 기기는 15“ 2-WAY 풀레인지 라우드 스피커로써 BGM 재생 및 레스토랑, 호텔 연회장 등 다양한 사이트에 설치가 가능하다. 90°×90°의 커버리지 패턴으로 균일하고 밸런스 잡힌 소리를 제공하며 DuraFlex 코팅 마감과 고강도 스틸 그릴로 외부 이물질로부터 인클로저 내부를 보호한다.

2) 기  능

- 15인치 고효율 로우 드라이버

- 90°×90° 커버리지 패턴

- 저왜곡 JBL 2408-2 고주파 압축 드라이버

- 15mm 합판으로 제작, DuraFlex TM 코팅 마감된 인클로저

- 손쉬운 운반을 위한 2개의 일체형 핸들

- 고강도 전면 그릴로 이물질로부터 보호

3) 사  양

- Frequency Range (-10 dB) : 45 Hz – 20 kHz

- Frequency Response (±3dB) : 75 Hz – 20 kHz

- Coverage : 90°×90°

- System Power Rating (IEC, 2 hrs) : 400 W / 800 W / 1600 W (continuous / music / peak)

- Maximum SPL (1m) : 125 dB continuous average (131 dB peak)

- System Sensitivity (2.83V@1m) : 99 dB

- Nominal Impedance : 8 Ω

- LF Driver : 1 × 15” woofer, 3” voice coil

- HF Driver : 1 × 2408-2, 1.5” voice coil, annular single diaphragm

- Enclosure : Trapezoidal with 20° side angles, 15mm poplar plywood, fitted with handles

- Suspension : 13 (3@top, 3@buttom, 2@each side, 3@rear) × M10 threaded hardware;
35mm  OmniMount pole-mounting socket

- Color : Black DuraFlexTM finish

- Enclosure Construction : Powder coated, 1.5 mm perforated steel

- Input Connector : NL4 Neutrik Speakon® in parallel for loop-through

- Dimensions (H×W D) : 680 × 414.4 × 445 mm

- Weight : 23.15 kg