LOUDSPEAKER (CV3025/66)

1) 용  도

본 기기는 듀얼 15“ 2-WAY 풀레인지 라우드 스피커로써 BGM 재생 및 레스토랑, 호텔 연회장 등 다양한 사이트에 설치가 가능하다. 60°×60°의 커버리지 패턴으로 균일하고 밸런스 잡힌 소리를 제공하며 DuraFlex 코팅 마감과 고강도 스틸 그릴로 외부 이물질로부터 인클로저 내부를 보호한다.

2) 기  능

- 듀얼 15인치 고효율 로우 드라이버

- 60°×60° 커버리지 패턴

- 저왜곡 JBL 2408H-1 고주파 압축 드라이버

- 합판으로 제작, DuraFlex TM 코팅 마감된 인클로저

- 손쉬운 운반을 위한 2개의 일체형 핸들

- 고강도 전면 그릴로 이물질로부터 보호

3) 사  양

- Frequency Range (-10 dB) : 42 Hz – 20 kHz

- FREQUENCY RESPONSE (±3dB) : 65 Hz – 18 kHz

- Coverage : 60°×60°

- System Power Rating : 800 W / 1600 W / 3200 W (continous / music / peak)

- Maximum SPL : 130 dB continuous average (136 dB peak)

- System Sensitivity (2.83V@1m) : 101 dB

- Nominal Impedance : 4 Ω

- LF Driver : 2 × 15” woofer

- HF Driver : 1 × 2408H-1

- Enclosure : Trapezoidal,15mm/18mm poplar plywood, fitted with handles

- Suspension : 13 (3@top, 3@buttom, 2@each side, 3@rear) × M10 threaded hardware

- Finish : Black DuraFlexTM finish

- Enclosure Construction : Powder coated, 1.5 mm perforated steel

- Input Connector : 2 × NL4 Neutrik Speakon®

- Dimensions (H×W×D) : 1243 × 484 × 520 mm

- Weight : 44.3 kg