ALL-IN-ONE RECHARGEABLE PA SOLUTION (EON ONE PRO)

1) 용  도

본 기기는 휴대용, 배터리 구동식 리니어 어레이 스피커이다. 컴팩트한 디자인과 충전식 리튬 이온 배터리로 최대 6시간의 재생 시간을 제공한다. 7채널 아날로그 믹서를 통해 깨끗한 음질을 구현하며 모바일 장치에서 블루투스를 통하여 음향 소스를 출력할 수 있다.

2) 기  능

- 6시간 배터리 사용 시간

- 초경량의 휴대용 스피커 시스템

- 무선 블루투스 스트리밍

- 7채널의 믹서 내장

- 휴대 기기로 전원 ON/OFF (USB 충전 포트 내장)

- 8“ 서브우퍼 및 리니어 디자인

3) 사  양

- System Type : Battery-operated portable line array with powered mixer

- Frequency Range (-10dB) : 37.5Hz ~ 18.5kHz

- Frequency Response (-3dB) : 45Hz ~ 18kHz

- Maximum SPL Output : 118 dB peak

- Speaker Driver : LF 1 x 8", HF 6 x 2"

- Speaker Coverage : 80° x 60° (H x V)

- Mixer : Seven-channel with Bluetooth streaming audio
streaming audio, (4) 1/4”/XLR, (1) 3.5 mm,(1) stereo RCA,
+48V phantom power, Hi-Z, and a pass-thru XLR connector

- Amp System Power Rating : 250W LF/HF

- AC input : 100 – 120 VAC, 50/60Hz; 220 – 240 VAC, 50/60Hz

- USB Power Port : Supplies 500mA

- Battery Type : Extended-life lithium-ion

- Battery Charge Time : 5 hours

- Battery Run Time : Up to 6 hours

- Unit Dimensions (D x W x H)mm : 401 x 266 x 594

- Packaged Dimensions (D x W x H)mm : 421 x 541 x 772

- Net Weight of System: 17 kg